HG D7 Cell VP16 .MAP

Results may vary, after a month of running with new cell and after a water cell flushing clean out
the cell efficiently goes up. Judge by the sound of the bubbles in the water tank. If  bubble rate
increase you will have to turn down the duty cycle% average and make a new .map in the VP16
programming. You want to enhance the combustion, NOT fight the engine timing and fight the
combustion ratter than enhance it. 90% of the time, less gas is better

Engine RPMs to Duty Cycle %(Amps)

  RPM - DC% - amps
———————
  200 - 10% - 1.0
  400 - 15% - 1.8
  600 - 20% - 2.7
  800 - 30% - 4.4
1000 - 35% - 5.3
1200 - 40% - 6.1
1400 - 45% - 7.0
1600 - 50% - 7.4
1800 - 50% - 7.4
2000 - 55% - 8.3
2200 - 55% - 8.3
2400 - 58% - 8.6
2600 - 60% - 9.0
2800 - 62% - 9.7
3000 - 65% - 9.8
3200 - 68% - 9.9
3400 - 70% - 10.0
3600 - 72% - 10.5
3800 - 75% - 11.4
4000 - 75% - 11.4
and up 75% - 11.4
——————

S7 Cell VP16 .MAP

Engine RPMs to Duty Cycle %(Amps)

  RPM - DC%
———————
  200 - 10% - .5
  400 - 15% - 1.0
  600 - 20% - 1.5
  800 - 30% - 2.5
1000 - 30% - 2.5
1200 - 35% - 3.0
1400 - 40% - 4.0
1600 - 40% - 4.0
1800 - 45% - 4.5
2000 - 55% - 5.0
2200 - 55% - 5.0
2400 - 58%  - 5.5
2600 - 60% - 6.0
2800 - 60% - 6.0
3000 - 60% - 6.0
3200 - 60% - 6.0
3400 - 60% - 6.0
3600 - 60% - 6.0
3800 - 62% - 6.2
4000 - 62% - 6.2
and up 65% - 6.8
——————